|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions
reset.c File Reference
MPLABX MCC Melody Code Generator » Reset Driver

This is the generated driver source file for RESET driver. More...

`#include <stdbool.h>`
`#include <stdint.h>`
`#include <xc.h>`
`#include "../reset.h"`
Include dependency graph for reset.c:

Go to the source code of this file.

## Functions
static bool | RESET_CauseFromTrap (uint16_t resetCause)
| RESET cause from trap.
static bool | RESET_CauseFromIllegalOpcode (uint16_t resetCause)
| RESET cause from Illegal Opcode
static bool | RESET_CauseFromConfigurationMismatch (uint16_t resetCause)
| RESET cause from Configuration Mismatch
static bool | RESET_CauseFromExternal (uint16_t resetCause)
| RESET cause from External
static bool | RESET_CauseFromSoftware (uint16_t resetCause)
| RESET cause from Software
static bool | RESET_CauseFromWatchdogTimer (uint16_t resetCause)
| RESET cause from Watchdog Time
static void | RESET_CauseClear (enum RESET_MASKS resetFlagMask)
| RESET cause from Clear
uint16_t | RESET_CauseGet (void)
| Returns the cause of previous reset.
void | __attribute__ ((weak))
void | RESET_CauseClearAll (void)
| Clears the Reset Cause register.

## Detailed Description

RESET Generated Driver Source File

Definition in file reset.c.

## Function Documentation

## ◆ __attribute__()

void __attribute__ | ( | (weak) |  | ) |

Definition at line 163 of file reset.c.

Here is the call graph for this function: