|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions | Variables
pwm.c File Reference
MPLABX MCC Melody Code Generator » PWM HS Driver

This is the generated driver source file for PWM driver. More...

`#include "../pwm.h"`
Include dependency graph for pwm.c:

Go to the source code of this file.

## Functions
void | PWM_Initialize (void)
| Initializes PWM module, using the given initialization data.
void | PWM_Deinitialize (void)
| Deinitializes the PWM to POR values.
void | PWM_GeneratorEOCEventCallbackRegister (void(*callback)(enum PWM_GENERATOR genNum))
| This function can be used to override default callback PWM_GeneratorEOCEventCallback and to define custom callback for PWM EOCEvent event.
void | __attribute__ ((weak))
void | PWM_GeneratorTasks (enum PWM_GENERATOR intGen)
| This is a tasks function for PWM1.

## Variables
static void(* | PWM_GeneratorEOCEventHandler )(enum PWM_GENERATOR genNum) = NULL
const struct PWM_HS_INTERFACE | PWM_HS
| Structure object of type PWM_HS_INTERFACE with the custom name given by the user in the Melody Driver User interface. The default name e.g. PWM_HS can be changed by the user in the PWM user interface. This allows defining a structure with application specific name using the 'Custom Name' field. Application specific name allows the API Portability.

## Detailed Description

PWM Generated Driver Source File

Definition in file pwm.c.

## Function Documentation

## ◆ __attribute__()

void __attribute__ | ( | (weak) |  | ) |

Definition at line 519 of file pwm.c.

## Variable Documentation

## ◆ PWM_GeneratorEOCEventHandler

void(* PWM_GeneratorEOCEventHandler) (enum PWM_GENERATOR genNum) | ( | enum PWM_GENERATOR | genNum | ) | = NULL
| static

Definition at line 45 of file pwm.c.