|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions
drv_custom_config_adc.h File Reference
Driver Layer » MCC Custom Code ADC

Contains ADC initialization that was not supported by MCC generated code.
More...

`#include "adc/adc1.h"`
`#include "drv_mcc_extension_adc.h"`
Include dependency graph for drv_custom_config_adc.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | ADC_CHANNEL_VSEC (2)
| ADC2 is routed to Secondary Voltage.
#define | ADC_CHANNEL_IPRI_CT (7)
| ADC7 is routed to Primary CT Current.
#define | ADC_CHANNEL_VPRI (10)
| ADC10 is routed to Primary Voltage.
#define | ADC_CHANNEL_TEMP (14)
| ADC14 is routed to Temperature.
#define | ADC_CHANNEL_VRAIL_5V (19)
| ADC19 is routed to 5V rail.
#define | ADC_CHANNEL_ISEC_CT (0)
| ADC0 is routed to Secondary CT Current.
#define | ADC_CHANNEL_ISEC_AVG (1)
| ADC1 is routed to Secondary Average Current.

## Functions
static __inline__ void | DRV_Config_Custom_ADC (void)
| Customize configuration for ADC.

## Detailed Description

<>

Definition in file drv_custom_config_adc.h.