|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Macros | Functions | Variables
cmp1.h File Reference
MPLABX MCC Melody Code Generator » CMP DAC Driver

This is the generated driver header file for the CMP1 driver. More...

`#include <stddef.h>`
`#include <stdbool.h>`
`#include "cmp_interface.h"`
Include dependency graph for cmp1.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | CMP_ISEC_SC_Initialize CMP1_Initialize
| This macro defines the Custom Name for CMP1_Initialize API.
#define | CMP_ISEC_SC_Deinitialize CMP1_Deinitialize
| This macro defines the Custom Name for CMP1_Deinitialize API.
#define | CMP_ISEC_SC_StatusGet CMP1_StatusGet
| This macro defines the Custom Name for CMP1_StatusGet API.
#define | CMP_ISEC_SC_Enable CMP1_Enable
| This macro defines the Custom Name for CMP1_Enable API.
#define | CMP_ISEC_SC_Disable CMP1_Disable
| This macro defines the Custom Name for CMP1_Disable API.
#define | CMP_ISEC_SC_DACEnable CMP1_DACEnable
| This macro defines the Custom Name for CMP1_DACEnable API.
#define | CMP_ISEC_SC_DACDisable CMP1_DACDisable
| This macro defines the Custom Name for CMP1_DACDisable API.
#define | CMP_ISEC_SC_DACDataWrite CMP1_DACDataWrite
| This macro defines the Custom Name for CMP1_DACDataWrite API.
#define | CMP_ISEC_SC_DACDisable CMP1_DACDisable
| This macro defines the Custom Name for CMP1_DACDisable API.
#define | CMP_ISEC_SC_EventCallbackRegister CMP1_EventCallbackRegister
| This macro defines the Custom Name for CMP1_EventCallbackRegister API.
#define | CMP_ISEC_SC_Tasks CMP1_Tasks
| This macro defines the Custom Name for CMP1_Tasks API.

## Functions
void | CMP1_Initialize (void)
| Initialize the CMP1 module.
void | CMP1_Deinitialize (void)
| Deinitializes the CMP1 to POR values.
bool | CMP1_StatusGet (void)
| Returns the comparator output status.
void | CMP1_Enable (void)
| Enables the common DAC module.
void | CMP1_Disable (void)
| Disables the common DAC module.
void | CMP1_DACEnable (void)
| Enables the individual DAC module.
void | CMP1_DACDisable (void)
| Disables the individual DAC module.
void | CMP1_DACDataWrite (size_t value)
| CMP DAC Data write to register.
void | CMP1_EventCallbackRegister (void(*handler)(void))
| This function can be used to override default callback and to define custom callback for CMP1 Event event.
void | CMP1_EventCallback (void)
| This is the default callback with weak attribute. The user can override and implement the default callback without weak attribute or can register a custom callback function using CMP1_EventCallbackRegister.
void | CMP1_Tasks (void)
| The Task function can be called in the main application using the High Speed Comparator, when interrupts are not used. This would thus introduce the polling mode feature of the Analog Comparator.

## Variables
const struct CMP_INTERFACE | CMP_ISEC_SC
| Structure object of type CMP_INTERFACE with the custom name given by the user in the Melody Driver User interface. The default name e.g. CMP_DAC1 can be changed by the user in the CMP user interface. This allows defining a structure with application specific name using the 'Custom Name' field. Application specific name allows the API Portability.

## Detailed Description

CMP1 Generated Driver Header File

Definition in file cmp1.h.