|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
reset_types.h
Go to the documentation of this file.
1
17/*
18© [2024] Microchip Technology Inc. and its subsidiaries.
19
20 Subject to your compliance with these terms, you may use Microchip
21 software and any derivatives exclusively with Microchip products.
22 You are responsible for complying with 3rd party license terms
23 applicable to your use of 3rd party software (including open source
24 software) that may accompany Microchip software. SOFTWARE IS ?AS IS.?
25 NO WARRANTIES, WHETHER EXPRESS, IMPLIED OR STATUTORY, APPLY TO THIS
26 SOFTWARE, INCLUDING ANY IMPLIED WARRANTIES OF NON-INFRINGEMENT,
27 MERCHANTABILITY, OR FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT
28 WILL MICROCHIP BE LIABLE FOR ANY INDIRECT, SPECIAL, PUNITIVE,
29 INCIDENTAL OR CONSEQUENTIAL LOSS, DAMAGE, COST OR EXPENSE OF ANY
30 KIND WHATSOEVER RELATED TO THE SOFTWARE, HOWEVER CAUSED, EVEN IF
31 MICROCHIP HAS BEEN ADVISED OF THE POSSIBILITY OR THE DAMAGES ARE
32 FORESEEABLE. TO THE FULLEST EXTENT ALLOWED BY LAW, MICROCHIP?S
33 TOTAL LIABILITY ON ALL CLAIMS RELATED TO THE SOFTWARE WILL NOT
34 EXCEED AMOUNT OF FEES, IF ANY, YOU PAID DIRECTLY TO MICROCHIP FOR
35 THIS SOFTWARE.
36*/
37
38#ifndef RESET_TYPES_H
39#define RESET_TYPES_H
40
46 enum RESET_TYPES
47{
48 RESET_ERROR_RCON_TRAPR = 1,
49 RESET_ERROR_RCON_IOPUWR = 2,
50 RESET_ERROR_RCON_CM = 3,
51 RESET_ERROR_RCON_WDTO_ISR = 4
52};
53
59 enum RESET_MASKS
60{
61 RESET_MASK_POR = 0x0001,
62 RESET_MASK_WDTO = 0x0010,
63 RESET_MASK_SWR = 0x0040,
64 RESET_MASK_EXTR = 0x0080,
65 RESET_MASK_CM = 0x0200,
66 RESET_MASK_IOPUWR = 0x4000,
67 RESET_MASK_TRAPR = 0x8000,
68};
69
70#endif /* RESET_TYPES_H */
71
RESET_MASKS
RESET_MASKS
Definition reset_types.h:60
RESET_MASK_WDTO
@ RESET_MASK_WDTO
Definition reset_types.h:62
RESET_MASK_EXTR
@ RESET_MASK_EXTR
Definition reset_types.h:64
RESET_MASK_SWR
@ RESET_MASK_SWR
Definition reset_types.h:63
RESET_MASK_CM
@ RESET_MASK_CM
Definition reset_types.h:65
RESET_MASK_IOPUWR
@ RESET_MASK_IOPUWR
Definition reset_types.h:66
RESET_MASK_TRAPR
@ RESET_MASK_TRAPR
Definition reset_types.h:67
RESET_MASK_POR
@ RESET_MASK_POR
Definition reset_types.h:61
RESET_TYPES
RESET_TYPES
Definition reset_types.h:47
RESET_ERROR_RCON_WDTO_ISR
@ RESET_ERROR_RCON_WDTO_ISR
Definition reset_types.h:51
RESET_ERROR_RCON_CM
@ RESET_ERROR_RCON_CM
Definition reset_types.h:50
RESET_ERROR_RCON_IOPUWR
@ RESET_ERROR_RCON_IOPUWR
Definition reset_types.h:49
RESET_ERROR_RCON_TRAPR
@ RESET_ERROR_RCON_TRAPR
Definition reset_types.h:48