|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Modules
Primary Voltage Feedback
Configuration Layer

Declaration of Primary Voltage Feedback parameters, fault configuration and macros. More...

Collaboration diagram for Primary Voltage Feedback:

## Modules
| Conversion Macros
| Conversion macros for user-declarations of Primary Voltage Feedback parameters.
#define | VPRI_OV_THRES_TRIG_VOLTS (float)(700.0)
#define | VPRI_OV_THRES_CLEAR_VOLTS (float)(600.0)
#define | VPRI_OV_T_BLANK_TRIG_SEC (float) (0.0)
#define | VPRI_OV_T_BLANK_CLEAR_SEC (float) (0.0)
#define | VPRI_OV_TICK_SEC (T_ADC_SAMPLE_SECS)
#define | VPRI_UV_THRES_TRIG_VOLTS (float)(300.0)
#define | VPRI_UV_THRES_CLEAR_VOLTS (float)(200.0)
#define | VPRI_UV_T_BLANK_TRIG_SEC (float) (0.0)
#define | VPRI_UV_T_BLANK_CLEAR_SEC (float) (0.0)
#define | VPRI_UV_TICK_SEC (T_ADC_SAMPLE_SECS)
#define | VPRI_SNS_GAIN (float)(3.600e-3)
#define | VPRI_SNS_OFS (0.0)
#define | VPRI_VOLTAGE_GAIN (float)0.2229

## Detailed Description

Declaration of Primary Voltage Feedback parameters, fault configuration and macros

## Macro Definition Documentation

## ◆ VPRI_OV_T_BLANK_CLEAR_SEC

#define VPRI_OV_T_BLANK_CLEAR_SEC (float) (0.0)

Definition at line 106 of file config.h.

## ◆ VPRI_OV_T_BLANK_TRIG_SEC

#define VPRI_OV_T_BLANK_TRIG_SEC (float) (0.0)

Definition at line 105 of file config.h.

## ◆ VPRI_OV_THRES_CLEAR_VOLTS

#define VPRI_OV_THRES_CLEAR_VOLTS (float)(600.0)

Definition at line 100 of file config.h.

## ◆ VPRI_OV_THRES_TRIG_VOLTS

#define VPRI_OV_THRES_TRIG_VOLTS (float)(700.0)

Definition at line 99 of file config.h.

## ◆ VPRI_OV_TICK_SEC

#define VPRI_OV_TICK_SEC (T_ADC_SAMPLE_SECS)

Definition at line 107 of file config.h.

## ◆ VPRI_SNS_GAIN

#define VPRI_SNS_GAIN (float)(3.600e-3)

Definition at line 19 of file hardware.h.

## ◆ VPRI_SNS_OFS

#define VPRI_SNS_OFS (0.0)

Definition at line 20 of file hardware.h.

## ◆ VPRI_UV_T_BLANK_CLEAR_SEC

#define VPRI_UV_T_BLANK_CLEAR_SEC (float) (0.0)

Definition at line 117 of file config.h.

## ◆ VPRI_UV_T_BLANK_TRIG_SEC

#define VPRI_UV_T_BLANK_TRIG_SEC (float) (0.0)

Definition at line 116 of file config.h.

## ◆ VPRI_UV_THRES_CLEAR_VOLTS

#define VPRI_UV_THRES_CLEAR_VOLTS (float)(200.0)

Definition at line 111 of file config.h.

## ◆ VPRI_UV_THRES_TRIG_VOLTS

#define VPRI_UV_THRES_TRIG_VOLTS (float)(300.0)

Definition at line 110 of file config.h.

## ◆ VPRI_UV_TICK_SEC

#define VPRI_UV_TICK_SEC (T_ADC_SAMPLE_SECS)

Definition at line 118 of file config.h.

## ◆ VPRI_VOLTAGE_GAIN

#define VPRI_VOLTAGE_GAIN (float)0.2229

Definition at line 23 of file hardware.h.