|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Modules
Temperature Feedback
Configuration Layer

Declaration of Temperature Feedback parameters. More...

Collaboration diagram for Temperature Feedback:

## Modules
| Conversion Macros
| Conversion macros for user-declarations of Temperature Feedback parameters details Conversion macros converting physical quantities of parameters into binary (integer) numbers for registers and variables.
#define | TEMPERATURE_PBV_OFFSET_CELSIUS (40u)
| To allow the PBV to support up to -40C, an offset was added.
#define | OTP_THRES_TRIG_CELCIUS (80u)
| Degrees Celcius.
#define | OTP_THRES_CLEAR_CELCIUS (70u)
| Degrees Celcius.
#define | FAULT_PERSISTENCE_COUNT_TEMP (4u)
#define | NOMINAL_TEMPERATURE_THRESHOLD (float) (40.0)
#define | TEMPERATURE_HYSTERESIS (float) (1.0)
| Degrees Celcius.
#define | TEMPERATURE_GAIN (-0.029)
#define | TEMPERATURE_OFFSET 115u

## Detailed Description

Declaration of Temperature Feedback parameters

## Macro Definition Documentation

## ◆ FAULT_PERSISTENCE_COUNT_TEMP

#define FAULT_PERSISTENCE_COUNT_TEMP (4u)

Definition at line 169 of file config.h.

## ◆ NOMINAL_TEMPERATURE_THRESHOLD

#define NOMINAL_TEMPERATURE_THRESHOLD (float) (40.0)

Definition at line 173 of file config.h.

## ◆ OTP_THRES_CLEAR_CELCIUS

#define OTP_THRES_CLEAR_CELCIUS (70u)

Definition at line 168 of file config.h.

## ◆ OTP_THRES_TRIG_CELCIUS

#define OTP_THRES_TRIG_CELCIUS (80u)

Definition at line 167 of file config.h.

## ◆ TEMPERATURE_GAIN

#define TEMPERATURE_GAIN (-0.029)

Definition at line 72 of file hardware.h.

## ◆ TEMPERATURE_HYSTERESIS

#define TEMPERATURE_HYSTERESIS (float) (1.0)

Definition at line 174 of file config.h.

## ◆ TEMPERATURE_OFFSET

#define TEMPERATURE_OFFSET 115u

Definition at line 73 of file hardware.h.

## ◆ TEMPERATURE_PBV_OFFSET_CELSIUS

#define TEMPERATURE_PBV_OFFSET_CELSIUS (40u)

Definition at line 166 of file config.h.