|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Conversion Macros
Configuration Layer » Temperature Feedback

Conversion macros for user-declarations of Temperature Feedback parameters details Conversion macros converting physical quantities of parameters into binary (integer) numbers for registers and variables. More...

Collaboration diagram for Conversion Macros:

#define | TEMPERATURE_FACTOR (int16_t)(TEMPERATURE_GAIN * pow(2.0, 15))
#define | L_TEMPERATURE_THRESHOLD (uint16_t)(NOMINAL_TEMPERATURE_THRESHOLD - TEMPERATURE_HYSTERESIS)
#define | H_TEMPERATURE_THRESHOLD (uint16_t)(NOMINAL_TEMPERATURE_THRESHOLD + TEMPERATURE_HYSTERESIS)

## Detailed Description

## Macro Definition Documentation

## ◆ H_TEMPERATURE_THRESHOLD

#define H_TEMPERATURE_THRESHOLD (uint16_t)(NOMINAL_TEMPERATURE_THRESHOLD + TEMPERATURE_HYSTERESIS)

Definition at line 157 of file macros.h.

## ◆ L_TEMPERATURE_THRESHOLD

#define L_TEMPERATURE_THRESHOLD (uint16_t)(NOMINAL_TEMPERATURE_THRESHOLD - TEMPERATURE_HYSTERESIS)

Definition at line 156 of file macros.h.

## ◆ TEMPERATURE_FACTOR

#define TEMPERATURE_FACTOR (int16_t)(TEMPERATURE_GAIN * pow(2.0, 15))

Definition at line 154 of file macros.h.