|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Typedefs | Enumerations
system_types.h File Reference
MPLABX MCC Melody Code Generator » System Driver

This is the generated driver types header file for the System driver. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Typedefs
typedef enum CORCON_MODE_TYPE | SYSTEM_CORCON_MODES

## Enumerations
enum | CORCON_MODE_TYPE { CORCON_MODE_PORVALUES = 0x0020 , CORCON_MODE_ENABLEALLSATNORMAL_ROUNDBIASED = 0x00E2 , CORCON_MODE_ENABLEALLSATNORMAL_ROUNDUNBIASED = 0x00E0 , CORCON_MODE_DISABLEALLSAT_ROUNDBIASED = 0x0022 , CORCON_MODE_DISABLEALLSAT_ROUNDUNBIASED = 0x0020 , CORCON_MODE_ENABLEALLSATSUPER_ROUNDBIASED = 0x00F2 , CORCON_MODE_ENABLEALLSATSUPER_ROUNDUNBIASED = 0x00F0 }

## Detailed Description

MAIN Generated Driver Types Header File

Version
  Driver Version 1.0.1

Definition in file system_types.h.

## Typedef Documentation

## ◆ SYSTEM_CORCON_MODES

typedef enum CORCON_MODE_TYPE SYSTEM_CORCON_MODES

## Enumeration Type Documentation

## ◆ CORCON_MODE_TYPE

enum CORCON_MODE_TYPE

Enumerator
CORCON_MODE_PORVALUES | Use POR values of CORCON
CORCON_MODE_ENABLEALLSATNORMAL_ROUNDBIASED | Enable saturation for ACCA, ACCB and Dataspace write, enable normal ACCA/ACCB saturation mode and set rounding to Biased (conventional) mode. Rest of CORCON settings are set to the default POR values.
CORCON_MODE_ENABLEALLSATNORMAL_ROUNDUNBIASED | Enable saturation for ACCA, ACCB and Dataspace write, enable normal ACCA/ACCB saturation mode and set rounding to Unbiased (convergent) mode. Rest of CORCON settings are set to the default POR values.
CORCON_MODE_DISABLEALLSAT_ROUNDBIASED | Disable saturation for ACCA, ACCB and Dataspace write and set rounding to Biased (conventional) mode. Rest of CORCON settings are set to the default POR values.
CORCON_MODE_DISABLEALLSAT_ROUNDUNBIASED | Disable saturation for ACCA, ACCB and Dataspace write and set rounding to Unbiased (convergent) mode. Rest of CORCON settings are set to the default POR values.
CORCON_MODE_ENABLEALLSATSUPER_ROUNDBIASED | Enable saturation for ACCA, ACCB and Dataspace write, enable super ACCA/ACCB saturation mode and set rounding to Biased (conventional) mode. Rest of CORCON settings are set to the default POR values.
CORCON_MODE_ENABLEALLSATSUPER_ROUNDUNBIASED | Enable saturation for ACCA, ACCB and Dataspace write, enable super ACCA/ACCB saturation mode and set rounding to Unbiased (convergent) mode. Rest of CORCON settings are set to the default POR values.

Definition at line 48 of file system_types.h.