BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_FLAGS Class Reference

Flags that provide information on the FTDI device state More...

## Public Attributes
const UInt32 | FT_FLAGS_OPENED = 0x00000001
| Indicates that the device is open More...
const UInt32 | FT_FLAGS_HISPEED = 0x00000002
| Indicates that the device is enumerated as a hi-speed USB device More...

## Detailed Description

Flags that provide information on the FTDI device state

## Member Data Documentation

## ◆ FT_FLAGS_HISPEED

const UInt32 FTD2XX_NET.FTDI.FT_FLAGS.FT_FLAGS_HISPEED = 0x00000002

Indicates that the device is enumerated as a hi-speed USB device

## ◆ FT_FLAGS_OPENED

const UInt32 FTD2XX_NET.FTDI.FT_FLAGS.FT_FLAGS_OPENED = 0x00000001

Indicates that the device is open

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs