BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_FLOW_CONTROL Class Reference

Permitted flow control values for FTDI devices More...

## Public Attributes
const UInt16 | FT_FLOW_NONE = 0x0000
| No flow control More...
const UInt16 | FT_FLOW_RTS_CTS = 0x0100
| RTS/CTS flow control More...
const UInt16 | FT_FLOW_DTR_DSR = 0x0200
| DTR/DSR flow control More...
const UInt16 | FT_FLOW_XON_XOFF = 0x0400
| Xon/Xoff flow control More...

## Detailed Description

Permitted flow control values for FTDI devices

## Member Data Documentation

## ◆ FT_FLOW_DTR_DSR

const UInt16 FTD2XX_NET.FTDI.FT_FLOW_CONTROL.FT_FLOW_DTR_DSR = 0x0200

DTR/DSR flow control

## ◆ FT_FLOW_NONE

const UInt16 FTD2XX_NET.FTDI.FT_FLOW_CONTROL.FT_FLOW_NONE = 0x0000

No flow control

## ◆ FT_FLOW_RTS_CTS

const UInt16 FTD2XX_NET.FTDI.FT_FLOW_CONTROL.FT_FLOW_RTS_CTS = 0x0100

RTS/CTS flow control

## ◆ FT_FLOW_XON_XOFF

const UInt16 FTD2XX_NET.FTDI.FT_FLOW_CONTROL.FT_FLOW_XON_XOFF = 0x0400

Xon/Xoff flow control

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs