BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_PARITY Class Reference

Permitted parity values for FTDI devices More...

## Public Attributes
const byte | FT_PARITY_NONE = 0x00
| No parity More...
const byte | FT_PARITY_ODD = 0x01
| Odd parity More...
const byte | FT_PARITY_EVEN = 0x02
| Even parity More...
const byte | FT_PARITY_MARK = 0x03
| Mark parity More...
const byte | FT_PARITY_SPACE = 0x04
| Space parity More...

## Detailed Description

Permitted parity values for FTDI devices

## Member Data Documentation

## ◆ FT_PARITY_EVEN

const byte FTD2XX_NET.FTDI.FT_PARITY.FT_PARITY_EVEN = 0x02

Even parity

## ◆ FT_PARITY_MARK

const byte FTD2XX_NET.FTDI.FT_PARITY.FT_PARITY_MARK = 0x03

Mark parity

## ◆ FT_PARITY_NONE

const byte FTD2XX_NET.FTDI.FT_PARITY.FT_PARITY_NONE = 0x00

No parity

## ◆ FT_PARITY_ODD

const byte FTD2XX_NET.FTDI.FT_PARITY.FT_PARITY_ODD = 0x01

Odd parity

## ◆ FT_PARITY_SPACE

const byte FTD2XX_NET.FTDI.FT_PARITY.FT_PARITY_SPACE = 0x04

Space parity

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs