| BSL430.NET 1.3.4

Properties | List of all members
BSL430_NET.FirmwareTools.FwTools.FwNode Class Reference

Atomic unit which every firmware consits of representated by single byte with max 32-bit long address. More...

## Properties
byte | Data = 0xFF`[get, set]`
| Data is single data byte with associated 16-bit address Addr. More...
long | Addr = 0`[get, set]`
| Addr is address of Data byte, max 32-bit length is supported. More...

## Detailed Description

Atomic unit which every firmware consits of representated by single byte with max 32-bit long address.

## Property Documentation

## ◆ Addr

long BSL430_NET.FirmwareTools.FwTools.FwNode.Addr = 0
| get set

Addr is address of Data byte, max 32-bit length is supported.

## ◆ Data

byte BSL430_NET.FirmwareTools.FwTools.FwNode.Data = 0xFF
| get set

Data is single data byte with associated 16-bit address Addr.

The documentation for this class was generated from the following file:

- D:/PROJECTS/C#/BSL430.NET/src/BSL430.NET.FirmwareTools/FwTools.cs