BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_STOP_BITS Class Reference

Permitted stop bits for FTDI devices More...

## Public Attributes
const byte | FT_STOP_BITS_1 = 0x00
| 1 stop bit More...
const byte | FT_STOP_BITS_2 = 0x02
| 2 stop bits More...

## Detailed Description

Permitted stop bits for FTDI devices

## Member Data Documentation

## ◆ FT_STOP_BITS_1

const byte FTD2XX_NET.FTDI.FT_STOP_BITS.FT_STOP_BITS_1 = 0x00

1 stop bit

## ◆ FT_STOP_BITS_2

const byte FTD2XX_NET.FTDI.FT_STOP_BITS.FT_STOP_BITS_2 = 0x02

2 stop bits

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs