SayoriOS 0.3.3

Функции | Переменные
Файл floppy.c

Драйвер Floppy. Подробнее...

`#include <drv/disk/floppy.h>`
`#include <io/ports.h>`
`#include "sys/timer.h"`
`#include "mem/vmm.h"`
`#include "drv/disk/dpm.h"`
`#include "io/tty.h"`
`#include "sys/isr.h"`

См. исходные тексты.

## Функции
floppy_t | Floppy (int device)
void | irq_waitFloppy ()
int | _FloppyError (int Device, int Error)
void | _FloppyMotor (int device, int status)
int | _FloppyCMD (int device, char cmd)
unsigned char | _FloppyData (int device)
void | _FloppyCI (int device, int *st0, int *cyl)
int | _FloppyCalibrate (int device)
int | _FloppyReset (int device)
int | _FloppySeek (int device, unsigned cyli, int head)
int | _FloppyTrack (int device, unsigned cyl, FloppyMode dir)
void | addr_2_coff (uint32_t addr, uint16_t *cyl, uint32_t *offset, uint32_t *size)
int | _FloppyCache (int device, FloppyMode mode, unsigned int addr, unsigned int *offset, unsigned int *size)
size_t | _FloppyRead (int device, char *dst, uint32_t addr, uint32_t size)
| [Floppy] Чтение данных на устройство Подробнее...
size_t | _FloppyWrite (int device, const char *dst, uint32_t addr, uint32_t size)
void | _FloppyServiceA ()
void | _FloppyCheck ()
| Автоматическое обновление данных о FD.
size_t | _FloppyDPMWriteA (size_t Disk, uint64_t high_offset, uint64_t low_offset, size_t Size, void *Buffer)
size_t | _FloppyDPMReadA (size_t Disk, uint64_t high_offset, uint64_t low_offset, size_t Size, void *Buffer)
void | _FloppyPrint ()
void | initFloppy ()

## Переменные
bool | _FloppyDebug = false
floppy_t | floppy_data [2] = {0}
volatile bool | interrupted = false

## Подробное описание

Драйвер Floppy.

Автор
  Пиминов Никита (nikit.nosp@m.a.pi.nosp@m.minof.nosp@m.f@ya.nosp@m.ndex..nosp@m.ru)

Версия
  0.3.5

Дата
  2023-07-25

Авторство
  Copyright SayoriOS Team (c) 2022-2024

См. определение в файле floppy.c

## Функции

## ◆ _FloppyRead()

size_t _FloppyRead | ( | int | device,
|  | char * | dst,
|  | uint32_t | addr,
|  | uint32_t | size
| ) |  |

[Floppy] Чтение данных на устройство

Аргументы

  dst | - Данные, откуда выполнить чтение
  addr | - Адрес, откуда читать (0 - в начало)
  size | - Сколько считать данных

Возвращает
  int Количество записанных байт

См. определение в файле floppy.c строка 343

## ◆ _FloppyTrack()

int _FloppyTrack | ( | int | device,
|  | unsigned | cyl,
|  | FloppyMode | dir
| ) |  |

FDB не проходит проверку SEEK

См. определение в файле floppy.c строка 233