#N canvas 417 32 561 662 10;
#X obj 6 419 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 6 504 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 6 598 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 105 512 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 105 426 cnv 17 3 47 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 134 424 signal;
#X text 133 512 signal;
#X text 198 604 (none);
#X obj 6 627 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X msg 226 157 reset;
#X text 146 441 bang;
#X text 140 458 reset;
#X obj 105 533 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 133 533 signal;
#X obj 105 553 cnv 17 3 17 empty empty 2 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 105 574 cnv 17 3 17 empty empty 3 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 140 553 float;
#X text 140 576 float;
#X obj 208 128 bng 20 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X text 186 512 - minimum level since startup or last reset;
#X text 186 533 - maximum level since startup or last reset;
#X text 186 553 - on bang: minimum level since startup or last reset;
#X text 186 576 - on bang: maximum level since startup or last reset;
#X obj 105 480 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 134 480 signal;
#X obj 295 130 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 295 156 cyclone/click~;
#X text 316 129 reset;
#X obj 266 228 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 295 207 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 262 332 Minimum level;
#X text 292 279 Maximum level;
#X text 331 229 Minimum level;
#X text 359 207 Maximum level;
#N canvas 649 173 371 512 example 0;
#X text 128 21 normalize a signal;
#X obj 193 152 cyclone/minmax~;
#X obj 193 187 abs~;
#X obj 201 224 max~;
#X obj 171 262 /~;
#X msg 237 120 reset;
#X obj 171 69 noise~;
#X obj 186 344 vu 15 120 empty empty -1 -8 0 10 #404040 #000000 1 0;
#X obj 74 307 vu 15 120 empty empty -1 -8 0 10 #404040 #000000 1 0;
#N canvas 133 46 409 280 level 0;
#X obj 212 162 cyclone/atodb;
#X obj 51 229 outlet;
#X obj 212 232 outlet;
#X obj 212 43 inlet~;
#X obj 212 125 cyclone/peakamp~ 1;
#X obj 51 127 cyclone/average~ 64 rms;
#X obj 51 164 cyclone/atodb~;
#X obj 51 197 cyclone/snapshot~ 100;
#X connect 0 0 2 0;
#X connect 3 0 4 0;
#X connect 3 0 5 0;
#X connect 4 0 0 0;
#X connect 5 0 6 0;
#X connect 6 0 7 0;
#X connect 7 0 1 0;
#X restore 59 253 pd level;
#X obj 171 97 *~ 2;
#N canvas 133 46 409 280 level 0;
#X obj 212 162 cyclone/atodb;
#X obj 51 229 outlet;
#X obj 212 232 outlet;
#X obj 212 43 inlet~;
#X obj 212 125 cyclone/peakamp~ 1;
#X obj 51 127 cyclone/average~ 64 rms;
#X obj 51 164 cyclone/atodb~;
#X obj 51 197 cyclone/snapshot~ 100;
#X connect 0 0 2 0;
#X connect 3 0 4 0;
#X connect 3 0 5 0;
#X connect 4 0 0 0;
#X connect 5 0 6 0;
#X connect 6 0 7 0;
#X connect 7 0 1 0;
#X restore 171 291 pd level;
#X connect 1 0 2 0;
#X connect 1 1 3 1;
#X connect 2 0 3 0;
#X connect 3 0 4 1;
#X connect 4 0 11 0;
#X connect 5 0 1 0;
#X connect 6 0 10 0;
#X connect 9 0 8 0;
#X connect 9 1 8 1;
#X connect 10 0 4 0;
#X connect 10 0 1 0;
#X connect 10 0 9 0;
#X connect 11 0 7 0;
#X connect 11 1 7 1;
#X restore 468 303 pd example;
#X obj 208 182 cyclone/minmax~;
#X text 67 84 [minmax~] outputs the minimum and maximum values (as signals and floats) of an input signal since the startup or a reset.;
#X text 192 480 - a non-zero value resets minimum and maximum;
#X text 192 441 - outputs minimum and maximum on float outlets;
#X text 192 424 - an input signal to analyze;
#X text 192 458 - resets minimum and maximum (to current input value);
#X obj 68 227 vsl 17 80 -1 1 0 0 dfgj dkhkgk empty 0 -9 0 10 #dcdcdc #000000 #000000 0 1;
#X obj 68 135 osc~ 0.1;
#X obj 499 69 cyclone/dsponoff~;
#X obj 3 4 ./header minmax~;
#X text 22 61 Minimum/Maximum values of a signal;
#X obj 68 205 cyclone/snapshot~ 1;
#X floatatom 68 318 7 0 0 0 - - - 0;
#X obj 208 309 cyclone/snapshot~ 1;
#X floatatom 208 330 8 0 0 0 - - - 0;
#X obj 237 256 cyclone/snapshot~ 1;
#X floatatom 237 277 8 0 0 0 - - - 0;
#X text 76 371 see also:;
#X obj 413 383 open-else;
#X text 460 360 click;
#X msg 413 361 range~;
#X text 146 366 Plugdata users or those with ELSE can also use [else/range~] as an alternative., f 42;
#X connect 9 0 35 0;
#X connect 18 0 35 0;
#X connect 25 0 26 0;
#X connect 26 0 35 1;
#X connect 35 0 48 0;
#X connect 35 1 50 0;
#X connect 35 2 28 0;
#X connect 35 3 29 0;
#X connect 41 0 47 0;
#X connect 42 0 35 0;
#X connect 42 0 46 0;
#X connect 46 0 41 0;
#X connect 48 0 49 0;
#X connect 50 0 51 0;
#X connect 55 0 53 0;
