# TL-WR841N OpenWrt
Hacking TL-WR841N Hardware v11 To Support OpenWrt
Mission completed.
### Router Info
1. Hardware version : v11
2. Firmware Region : eu
3. 4 MB Flash
4. 32 MB Ram
### How To Do ?
1. First download the Freifunk firmware from /firmwares/custom/freifunk folder.
2. Rename it to firmware.bin
3. Flash the firmware via firmware upgrade option in router webpage via LAN.
4. If you choose openwrt images then they should be renamed to firmware.bin
